Processor: ARM926EJ-S rev 0 (v5l)
BogoMIPS: 956.82
Features: swp half thumb fastmult vfp edsp 
CPU implementer: 0x41
CPU architecture: 5TE
CPU variant: 0x1
CPU part: 0x926
CPU revision: 0
Cache type: write-back
Cache clean: cp15 c7 ops
Cache lockdown: format C
Cache format: Harvard
I size: 32768
I assoc: 4
I line length: 32
I sets: 256
D size: 32768
D assoc: 4
D line length: 32
D sets: 256

Hardware: Feroceon-MV78XX0
Revision: 0000
Serial: 0000000000000000
